| CE Gobi SDK 2.7 GobiApi

- Main Page
- Modules
- Classes
- Files

- Class List
- Class Index
- Class Members

Public Attributes | List of all members
extCallFWInfo Struct Reference

`#include <GobiVoiceMgmtAPI.h>`

## Public Attributes
BYTE | SvcStatus
BYTE | SvcClass
BYTE | noReplyTimer
BYTE | pi
BYTE | si
BYTE | numType
BYTE | numLen
CHAR | number [MAX_DESCRIPTION_LENGTH]

## Detailed Description

This structure contains information for Get Call Forwarding Information.

Parameters

  SvcStatus | Service status. Values: 0x00 - SERVICE_STATUS_INACTIVE - Inactive 0x01 - SERVICE_STATUS_ACTIVE - Active
  SvcClass | Service Class is a combination (sum) of information class constants See qaGobiApiTableSupServiceInfoClasses.h for service classes.
  numLen | Provides the length of number which follow.
  number[MAX_DESCRIPTION_LENGTH] | number of numLen length, NULL terminated.
  noReplyTimer | No reply timer value in seconds A value of 0 indicates that noReplyTimer is ignored.

The documentation for this struct was generated from the following file:

- GobiVoiceMgmtAPI.h