| CE Gobi SDK 2.7 GobiApi

- Main Page
- Modules
- Classes
- Files

- Class List
- Class Index
- Class Members

Public Attributes | List of all members
callBarringPwd Struct Reference

`#include <GobiVoiceMgmtAPI.h>`

## Public Attributes
BYTE | reason
CHAR | oldPwd [PASSWORD_LENGTH]
CHAR | newPwd [PASSWORD_LENGTH]
CHAR | newPwdAgain [PASSWORD_LENGTH]

## Detailed Description

This structure contains Voice Set Call Barring Password Request Parameters

Parameters

  Reason | Call Barring Reason Values: 0x07 - QMI_VOICE_REASON_BARR_ALLOUTGOING - All outgoing 0x08 - QMI_VOICE_REASON_BARR_OUTGOINGINT - Outgoing internal 0x09 - QMI_VOICE_REASON_BARR_OUTGOINGINTEXTOHOME - Outgoing external to home 0x0A - QMI_VOICE_REASON_BARR_ALLINCOMING - All incoming 0x0B - QMI_VOICE_REASON_BARR_INCOMINGROAMING - Roaming incoming 0x0C - QMI_VOICE_REASON_BARR_ALLBARRING - All calls are barred 0x0D - QMI_VOICE_REASON_BARR_ALLOUTGOINGBARRING - All outgoing calls are barred 0x0E - QMI_VOICE_REASON_BARR_ALLINCOMINGBARRING - All incoming calls are barred
  oldPasswd[PASSWORD_LENGTH] | Old password. Password consists of 4 ASCII digits. Range: 0000 to 9999.
  newPasswd[PASSWORD_LENGTH] | New password. Password consists of 4 ASCII digits. Range: 0000 to 9999.
  newPasswdAgain[PASSWORD_LENGTH] | New password Again. Password consists of 4 ASCII digits. Range: 0000 to 9999.

The documentation for this struct was generated from the following file:

- GobiVoiceMgmtAPI.h