| CE Gobi SDK 2.7 GobiApi

- Main Page
- Modules
- Classes
- Files

- Class List
- Class Index
- Class Members

Public Attributes | List of all members
curAMRConfig Struct Reference

`#include <GobiVoiceMgmtAPI.h>`

## Public Attributes
BYTE | gsmAmrStat
BYTE | wcdmaAmrStat

## Detailed Description

This structure contains the Current Adaptive Multi Rate Configuration Information.

Parameters

  gsmAmrStat | GSM AMR Status 0x00 - Disable 0x01 - Enable 0xFF - Not Available
  wcdmaAmrStat | WCDMA AMR Status One or a combination of the following bitmask values: Bit 0 - AMR codec advertised is not supported Bit 1 - Controls WCDMA AMR wideband Bit 2 - Controls GSM half rate AMR Bit 3 - Controls GSM AMR wideband Bit 4 - Controls GSM AMR narrowband 0xFF, if not available

The documentation for this struct was generated from the following file:

- GobiVoiceMgmtAPI.h