| CE Gobi SDK 2.7 GobiApi

- Main Page
- Modules
- Classes
- Files

- Class List
- Class Index
- Class Members

Public Attributes | List of all members
TrueImsi Struct Reference
Gobi Connection Mangement

`#include <GobiConnectionMgmtAPI.h>`

## Public Attributes
BYTE | mcc_t [MAX_MCC]
BYTE | imsi_t_11_12 [MAX_IMSI_11_12]
BYTE | imsi_t_s1 [MAX_IMSI_S1]
BYTE | imsi_t_s2 [MAX_IMSI_S2]
BYTE | imsi_t_addr_num

## Detailed Description

True IMSI (information written to NV_IMSI_T_MCC_I, NV_IMSI_T_11_12_I, NV_IMSI_T_S1_I, NV_IMSI_T_S2_I, and NV_IMSI_T_ADDR_NUM_I)

Parameters

  mcc_t | ASCII character representation of MCC_T; example: 000, 123, etc.
  imsi_t_11_12 | ASCII character representation of IMSI_T_11_12 value; example: 00, 01, etc.
  imsi_t_s1 | ASCII character representation of IMSI_T_S1 value; example: 0123456.
  imsi_t_s2 | ASCII character representation of IMSI_T_S2 value; example: 012.
  imsi_t_addr_num | Value of IMSI_T_ADDR_NUM.

The documentation for this struct was generated from the following file:

- GobiConnectionMgmtAPI.h