| CE Gobi SDK 2.7 GobiApi

- Main Page
- Modules
- Classes
- Files

- Class List
- Class Index
- Class Members

Public Attributes | List of all members
callFwdTypeAndPlan Struct Reference

`#include <GobiVoiceMgmtAPI.h>`

## Public Attributes
BYTE | numberType
BYTE | numberPlan

## Detailed Description

This structure contains Supplementary Service request parameters related to different features and their activation, deactivation, registration and erasure (applicable only for 3GPP)

Parameters

  numberType | Call forwarding number type 0x00 - QMI_VOICE_NUM_TYPE_UNKNOWN Unknown 0x01 - QMI_VOICE_NUM_TYPE_INTERNATIONAL International 0x02 - QMI_VOICE_NUM_TYPE_NATIONAL National 0x03 - QMI_VOICE_NUM_TYPE_NETWORK_SPECIFIC Network-specific 0x04 - QMI_VOICE_NUM_TYPE_SUBSCRIBER Subscriber 0x05 - QMI_VOICE_NUM_TYPE_RESERVED Reserved 0x06 - QMI_VOICE_NUM_TYPE_ABBREVIATED Abbreviated 0x07 - QMI_VOICE_NUM_TYPE_RESERVED_EXTENSION Reserved extension
  numberPlan | Call forwarding number plan 0x00 - QMI_VOICE_NUM_PLAN_UNKNOWN Unknown 0x01 - QMI_VOICE_NUM_PLAN_ISDN ISDN 0x03 - QMI_VOICE_NUM_PLAN_DATA Data 0x04 - QMI_VOICE_NUM_PLAN_TELEX Telex 0x08 - QMI_VOICE_NUM_PLAN_NATIONAL National 0x09 - QMI_VOICE_NUM_PLAN_PRIVATE Private 0x0B - QMI_VOICE_NUM_PLAN_RESERVED_CTS Reserved cordless telephony system 0x0F - QMI_VOICE_NUM_PLAN_RESERVED_EXTENSION Reserved extension

The documentation for this struct was generated from the following file:

- GobiVoiceMgmtAPI.h