| CE Gobi SDK 2.7 GobiApi

- Main Page
- Modules
- Classes
- Files

- Class List
- Class Index
- Class Members

Public Attributes | List of all members
UUSInfo Struct Reference

`#include <GobiVoiceMgmtAPI.h>`

## Public Attributes
BYTE | UUSType
BYTE | UUSDcs
BYTE | UUSDatalen
CHAR | UUSData [MAX_DESCRIPTION_LENGTH]

## Detailed Description

This structure contains User to User Signaling Service Information.

Parameters

  UUSType | UUS type values are: 0x00 - UUS_DATA 0x01 - UUS_TYPE1_IMPLICIT 0x02 - UUS_TYPE1_REQUIRED 0x03 - UUS_TYPE1_NOT_REQUIRED 0x04 - UUS_TYPE2_REQUIRED 0x05 - UUS_TYPE2_NOT_REQUIRED 0x06 - UUS_TYPE3_REQUIRED 0x07 - UUS_TYPE3_NOT_REQUIRED 0xFF - Not Available
  UUSDcs | UUS data coding scheme values are: 0x01 - UUS_DCS_USP 0x02 - UUS_DCS_OHLP 0x03 - UUS_DCS_X244 0x04 - UUS_DCS_SMCF 0x05 - UUS_DCS_IA5 0x06 - UUS_DCS_RV12RD 0x07 - UUS_DCS_Q931UNCCM 0xFF - Not Available
  UUSDatalen | Number of sets of the following elements. UUSData If zero(0) then no further information exists.
  UUSData[MAX_DESCRIPTION_LENGTH] | UUS data encoded as per coding scheme

The documentation for this struct was generated from the following file:

- GobiVoiceMgmtAPI.h