| CE Gobi SDK 2.7 GobiApi

- Main Page
- Modules
- Classes
- Files

- Class List
- Class Index
- Class Members

Public Attributes | List of all members
ccSUPSType Struct Reference

`#include <GobiVoiceMgmtAPI.h>`

## Public Attributes
BYTE | svcType
BYTE | reason

## Detailed Description

This structure contains information about the Call Control Supplementary Service Types

Parameters

  svcType | Service type. 0x01 - VOICE_CC_SUPS_RESULT_SERVICE_TYPE_ACTIVATE - Activate 0x02 - VOICE_CC_SUPS_RESULT_SERVICE_TYPE_DEACTIVATE - Deactivate 0x03 - VOICE_CC_SUPS_RESULT_SERVICE_TYPE_REGISTER - Register 0x04 - VOICE_CC_SUPS_RESULT_SERVICE_TYPE_ERASE - Erase 0x05 - VOICE_CC_SUPS_RESULT_SERVICE_TYPE_INTERROGATE - Interrogate 0x06 - VOICE_CC_SUPS_RESULT_SERVICE_TYPE_REGISTER_PASSWORD - Register password 0x07 - VOICE_CC_SUPS_RESULT_SERVICE_TYPE_USSD - USSD 0xFF - Not Available
  reason | Call control supplementary service result reason Values: See qaGobiApiTableCallControlReturnReasons.h for return reasons.

The documentation for this struct was generated from the following file:

- GobiVoiceMgmtAPI.h