| CE Gobi SDK 2.7 GobiApi

- Main Page
- Modules
- Classes
- Files

- Class List
- Class Index
- Class Members

Public Attributes | List of all members
ectInfo Struct Reference

`#include <GobiVoiceMgmtAPI.h>`

## Public Attributes
BYTE | ectCallState
BYTE | pi
BYTE | numLen
CHAR | number [MAX_DESCRIPTION_LENGTH]

## Detailed Description

This structure contains information of ECT number.

Parameters

  ectCallState | ECT call states 0x00 - ECT_CALL_STATE_NONE – None

- 0x01 - ECT_CALL_STATE_ALERTING – Alerting
- 0x02 - ECT_CALL_STATE_ACTIVE – Active

Parameters

  pi | Presentation indicator. 0x00 – presentationAllowedAddress 0x01 – presentationRestricted 0x02 – numberNotAvailable 0x04 – presentationRestrictedAddress
  numLen | Provides the length of number which follow. If zero(0) then no further information exists.
  number | Number in ASCII, NULL ending.

The documentation for this struct was generated from the following file:

- GobiVoiceMgmtAPI.h