| CE Gobi SDK 2.14 GobiApi

- Main Page
- Modules
- Classes
- Files

- Class List
- Class Index
- Class Members

Public Attributes | List of all members
voiceSetSUPSServiceReq Struct Reference

`#include <GobiVoiceMgmtAPI.h>`

## Public Attributes
BYTE | voiceSvc
BYTE | reason
BYTE * | pServiceClass
BYTE * | pCallBarringPasswd
BYTE * | pCallForwardingNumber
BYTE * | pTimerVal
callFwdTypeAndPlan * | pCallFwdTypeAndPlan

## Detailed Description

This structure contains Supplementary Service request parameters related to different features and their activation, deactivation, registration and erasure (applicable only for 3GPP)

Parameters

  voiceSvc | Manages all call-independent supplementary services, such as activation, deactivation, registration, and erasure (mandatory) 0x01 - VOICE_SERVICE_ACTIVATE 0x02 - VOICE_SERVICE_DEACTIVATE 0x03 - VOICE_SERVICE_REGISTER 0x04 - VOICE_SERVICE_ERASE
  reason | supplementary service reason values (mandatory) 0x01 - QMI_VOICE_REASON_FWD_UNCONDITIONAL Unconditional call forwarding 0x02 - QMI_VOICE_REASON_FWD_MOBILEBUSY Forward when the mobile is busy 0x03 - QMI_VOICE_REASON_FWD_NOREPLY Forward when there is no reply 0x04 - QMI_VOICE_REASON_FWD_UNREACHABLE Forward when the call is unreachable 0x05 - QMI_VOICE_REASON_FWD_ALLFORWARDING All forwarding 0x06 - QMI_VOICE_REASON_FWD_ALLCONDITIONAL All conditional forwarding 0x07 - QMI_VOICE_REASON_BARR_ALLOUTGOING All outgoing calls are barred 0x08 - QMI_VOICE_REASON_BARR_OUTGOINGINT Outgoing internal calls are barred 0x09 - QMI_VOICE_REASON_BARR_OUTGOINGINTEXTOHOME Outgoing calls external to home are barred 0x0A - QMI_VOICE_REASON_BARR_ALLINCOMING All incoming calls are barred 0x0B - QMI_VOICE_REASON_BARR_INCOMINGROAMING Roaming incoming calls are barred 0x0C - QMI_VOICE_REASON_BARR_ALLBARRING All calls are barred 0x0D - QMI_VOICE_REASON_BARR_ALLOUTGOINGBARRING All outgoing calls are barred 0x0E - QMI_VOICE_REASON_BARR_ALLINCOMINGBARRING All incoming calls are barred 0x0F - QMI_VOICE_REASON_CALLWAITING Call waiting
  pServiceClass | Service class is a combination (sum) of information class constants (optional) See serviceClassInformation for more information
  pCallBarringPasswd | Password is required if call barring is provisioned using a password. Password consists of 4 ASCII digits. Range: 0000 to 9999 (optional)
  pCallForwardingNumber | Call forwarding number to be registered with the network. This has to be included in the request only when the service is set to VOICE_SERVICE_REGISTER. NULL terminated ASCII string. (optional)
  pTimerVal | Call forwarding no reply timer value in seconds. This has to be included in the request only when the service is set to VOICE_SERVICE_REGISTER and the reason is QMI_VOICE_REASON_FWD_NOREPLY. (optional) Range: 5 to 30 in steps of 5
  pCallFwdTypeAndPlan | Information about call forwarding type and plan. This parameter is ignored when the Call Forwarding Number is not included (optional) See callFwdTypeAndPlan for more information

The documentation for this struct was generated from the following file:

- GobiVoiceMgmtAPI.h