| CE Gobi SDK 2.14 GobiApi

- Main Page
- Modules
- Classes
- Files

- Class List
- Class Index
- Class Members

Public Attributes | List of all members
DTMFInfo Struct Reference

`#include <GobiVoiceMgmtAPI.h>`

## Public Attributes
BYTE | callID
BYTE | DTMFEvent
BYTE | digitCnt
BYTE | digitBuff [MAX_DESCRIPTION_LENGTH]

## Detailed Description

This structure contains information about the DTMF (Dual Tone Multi-Frequency).

Parameters

  callID | Call identifier for the current call.
  DTMFEvent | DTMF event 0x00 - DTMF_EVENT_REV_BURST - Sends a CDMA-burst DTMF 0x01 - DTMF_EVENT_REV_START_CONT - Starts a continuous DTMF tone 0x03 - DTMF_EVENT_REV_STOP_CONT - Stops a continuous DTMF tone 0x05 - DTMF_EVENT_FWD_BURST - Received a CDMA-burst DTMF message 0x06 - DTMF_EVENT_FWD_START_CONT - Received a start-continuous DTMF tone order 0x07 - DTMF_EVENT_FWD_STOP_CONT - Received a stop-continuous DTMF tone order
  digitCnt | Number of set of following element i.e. digitBuff.
  digitBuff[MAX_DESCRIPTION_LENGTH] | DTMF digit buffer in ASCII string which is NULL terminated

The documentation for this struct was generated from the following file:

- GobiVoiceMgmtAPI.h