| CE Gobi SDK 2.14 GobiApi

- Main Page
- Modules
- Classes
- Files

- Class List
- Class Index
- Class Members

Public Attributes | List of all members
roamTimer Struct Reference

`#include <GobiVoiceMgmtAPI.h>`

## Public Attributes
BYTE | namID
ULONG | roamTimerValue

## Detailed Description

This structure contains information about the Roam Timer.

Parameters

  namID | Index of the NAM(Number Assignment Module) to be configured. Range 0 to 3. Some modems support only 1 or 2 NAMs. 0xFF,if not available.
  roamTimerValue | Time in minutes. Cumulative air time is slammed. 0xFFFFFFFF,if not available.

The documentation for this struct was generated from the following file:

- GobiVoiceMgmtAPI.h