| CE Gobi SDK 2.14 GobiApi

- Main Page
- Modules
- Classes
- Files

- Class List
- Class Index
- Class Members

Public Attributes | List of all members
MinBasedImsi Struct Reference
Gobi Connection Mangement

`#include <GobiConnectionMgmtAPI.h>`

## Public Attributes
BYTE | mcc_m [MAX_MCC]
BYTE | imsi_m_11_12 [MAX_IMSI_11_12]
BYTE | imsi_m_s1 [MAX_IMSI_S1]
BYTE | imsi_m_s2 [MAX_IMSI_S2]

## Detailed Description

MIN-based IMSI (information written to NV_IMSI_MCC_I, NV_IMSI_11_12_I, NV_MIN1_I, and NV_MIN2_I)

Parameters

  mcc_m | ASCII character representation of MCC_M; example: 000, 123, etc.
  imsi_m_11_12 | ASCII character representation of IMSI_M_11_12 value; example: 00, 01, etc.
  imsi_m_s1 | ASCII character representation of IMSI_M_S1 value; example: 0123456.
  imsi_m_s2 | ASCII character representation of IMSI_M_S2 value; example: 012.

The documentation for this struct was generated from the following file:

- GobiConnectionMgmtAPI.h